Topographic Map Foam Model

1. Cut the paper topo map on the North side– cut through the other contour lines to get to the middle of the map (the pond outline).
2. Cut the blue line all the way around, even though you will cut through some of the contour lines.
3. Take the map and lay it on the 1st piece of foam.
4. Trace the **INSIDE** line of the map.
5. Cut the inside of the foam out.
6. Take the paper map and cut the next line (Red) from the inside out. Make careful cuts.
7. Take the map and lay it on the 2nd piece of foam.
8. Trace the **INSIDE** line of the map.
9. Cut the inside of the foam out.
10. Take the paper map and cut the next line (Red) from the inside out. Make careful cuts.
11. Take the map and lay it on the 2nd piece of foam.
12. Trace the **INSIDE** line of the map.
13. Cut the inside of the foam out.
14. Continue cutting and tracing and cutting until you reach the outside of the map.